          Full Z80 Opcode List Including Undocumented Opcodes
          ===================================================
               File: DOCS.Comp.Z80.OpList - Update: 0.10
                Author: J.G.Harston - Date: 09-09-1997
    
nn nn             DD nn          CB nn       FD CB ff nn      ED nn
--------------------------------------------------------------------------
00 NOP            -              RLC  B      rlc (iy+0)->b    MOS_QUIT
01 LD   BC,&0000  -              RLC  C      rlc (iy+0)->c    MOS_CLI 
02 LD   (BC),A    -              RLC  D      rlc (iy+0)->d    MOS_BYTE
03 INC  BC        -              RLC  E      rlc (iy+0)->e    MOS_WORD
04 INC  B         -              RLC  H      rlc (iy+0)->h    MOS_WRCH
05 DEC  B         -              RLC  L      rlc (iy+0)->l    MOS_RDCH
06 LD   B,&00     -              RLC  (HL)   RLC  (IY+0)      MOS_FILE
07 RLCA           -              RLC  A      rlc (iy+0)->a    MOS_ARGS
08 EX   AF,AF'    -              RRC  B      rrc (iy+0)->b    MOS_BGET
09 ADD  HL,BC     ADD  IX,BC     RRC  C      rrc (iy+0)->c    MOS_BPUT
0A LD   A,(BC)    -              RRC  D      rrc (iy+0)->d    MOS_GBPB
0B DEC  BC        -              RRC  E      rrc (iy+0)->e    MOS_FIND
0C INC  C         -              RRC  H      rrc (iy+0)->h    MOS_FF0C
0D DEC  C         -              RRC  L      rrc (iy+0)->l    MOS_FF0D
0E LD   C,&00     -              RRC  (HL)   RRC  (IY+0)      MOS_FF0E
0F RRCA           -              RRC  A      rrc (iy+0)->a    MOS_FF0F
10 DJNZ &4546     -              RL   B      rl  (iy+0)->b    -
11 LD   DE,&0000  -              RL   C      rl  (iy+0)->c    -
12 LD   (DE),A    -              RL   D      rl  (iy+0)->d    -
13 INC  DE        -              RL   E      rl  (iy+0)->e    -
14 INC  D         -              RL   H      rl  (iy+0)->h    -
15 DEC  D         -              RL   L      rl  (iy+0)->l    -
16 LD   D,&00     -              RL   (HL)   RL   (IY+0)      -
17 RLA            -              RL   A      rl  (iy+0)->a    -
18 JR   &4546     -              RR   B      rr  (iy+0)->b    -
19 ADD  HL,DE     ADD  IX,DE     RR   C      rr  (iy+0)->c    -
1A LD   A,(DE)    -              RR   D      rr  (iy+0)->d    -
1B DEC  DE        -              RR   E      rr  (iy+0)->e    -
1C INC  E         -              RR   H      rr  (iy+0)->h    -
1D DEC  E         -              RR   L      rr  (iy+0)->l    -
1E LD   E,&00     -              RR   (HL)   RR   (IY+0)      -
1F RRA            -              RR   A      rr  (iy+0)->a    -
20 JR   NZ,&4546  -              SLA  B      sla (iy+0)->b    -
21 LD   HL,&0000  LD   IX,&0000  SLA  C      sla (iy+0)->c    -
22 LD  (&0000),HL LD  (&0000),IX SLA  D      sla (iy+0)->d    -
23 INC  HL        INC  IX        SLA  E      sla (iy+0)->e    -
24 INC  H         INC  IXH       SLA  H      sla (iy+0)->h    -
25 DEC  H         DEC  IXH       SLA  L      sla (iy+0)->l    -
26 LD   H,&00     LD   IXH,&00   SLA  (HL)   SLA  (IY+0)      -
27 DAA            -              SLA  A      sla (iy+0)->a    -
28 JR   Z,&4546   -              SRA  B      sra (iy+0)->b    -
29 ADD  HL,HL     ADD  IX,IX     SRA  C      sra (iy+0)->c    -
2A LD  HL,(&0000) LD  IX,(&0000) SRA  D      sra (iy+0)->d    -
2B DEC  HL        DEC  IX        SRA  E      sra (iy+0)->e    -
2C INC  L         INC  IXL       SRA  H      sra (iy+0)->h    -
2D DEC  L         DEC  IXL       SRA  L      sra (iy+0)->l    -
2E LD   L,&00     LD   IXL,&00   SRA  (HL)   SRA  (IY+0)      -
2F CPL            -              SRA  A      sra (iy+0)->a    -
30 JR   NC,&4546  -              SLS  B      sls (iy+0)->b    -
31 LD   SP,&0000  -              SLS  C      sls (iy+0)->c    -
32 LD   (&0000),A -              SLS  D      sls (iy+0)->d    -
33 INC  SP        -              SLS  E      sls (iy+0)->e    -
34 INC  (HL)      INC  (IX+0)    SLS  H      sls (iy+0)->h    -
35 DEC  (HL)      DEC  (IX+0)    SLS  L      sls (iy+0)->l    -
36 LD   (HL),&00  LD  (IX+0),&00 SLS  (HL)   SLS  (IY+0)      -
37 SCF            -              SLS  A      sls (iy+0)->a    -
38 JR   C,&4546   -              SRL  B      srl (iy+0)->b    -
39 ADD  HL,SP     ADD  IX,SP     SRL  C      srl (iy+0)->c    -
3A LD   A,(&0000) -              SRL  D      srl (iy+0)->d    -
3B DEC  SP        -              SRL  E      srl (iy+0)->e    -
3C INC  A         -              SRL  H      srl (iy+0)->h    -
3D DEC  A         -              SRL  L      srl (iy+0)->l    -
3E LD   A,&00     -              SRL  (HL)   SRL  (IY+0)      -
3F CCF            -              SRL  A      srl (iy+0)->a    -
40 LD   B,B       -              BIT  0,B    bit 0,(iy+0)->b  IN   B,(C)
41 LD   B,C       -              BIT  0,C    bit 0,(iy+0)->c  OUT  (C),B
42 LD   B,D       -              BIT  0,D    bit 0,(iy+0)->d  SBC  HL,BC
43 LD   B,E       -              BIT  0,E    bit 0,(iy+0)->e  LD   (&0000),BC
44 LD   B,H       LD   B,IXH     BIT  0,H    bit 0,(iy+0)->h  NEG
45 LD   B,L       LD   B,IXL     BIT  0,L    bit 0,(iy+0)->l  RETN
46 LD   B,(HL)    LD   B,(IX+0)  BIT  0,(HL) BIT  0,(IY+0)    IM   0
47 LD   B,A       -              BIT  0,A    bit 0,(iy+0)->a  LD   I,A
48 LD   C,B       -              BIT  1,B    bit 1,(iy+0)->b  IN   C,(C)
49 LD   C,C       -              BIT  1,C    bit 1,(iy+0)->c  OUT  (C),C
4A LD   C,D       -              BIT  1,D    bit 1,(iy+0)->d  ADC  HL,BC
4B LD   C,E       -              BIT  1,E    bit 1,(iy+0)->e  LD   BC,(&0000)
4C LD   C,H       LD   C,IXH     BIT  1,H    bit 1,(iy+0)->h  [neg]
4D LD   C,L       LD   C,IXL     BIT  1,L    bit 1,(iy+0)->l  RETI
4E LD   C,(HL)    LD   C,(IX+0)  BIT  1,(HL) BIT  1,(IY+0)    [im0]
4F LD   C,A       -              BIT  1,A    bit 1,(iy+0)->a  LD   R,A
50 LD   D,B       -              BIT  2,B    bit 2,(iy+0)->b  IN   D,(C)
51 LD   D,C       -              BIT  2,C    bit 2,(iy+0)->c  OUT  (C),D
52 LD   D,D       -              BIT  2,D    bit 2,(iy+0)->d  SBC  HL,DE
53 LD   D,E       -              BIT  2,E    bit 2,(iy+0)->e  LD   (&0000),DE
54 LD   D,H       LD   D,IXH     BIT  2,H    bit 2,(iy+0)->h  [neg]
55 LD   D,L       LD   D,IXL     BIT  2,L    bit 2,(iy+0)->l  [retn]
56 LD   D,(HL)    LD   D,(IX+0)  BIT  2,(HL) BIT  2,(IY+0)    IM   1
57 LD   D,A       -              BIT  2,A    bit 2,(iy+0)->a  LD   A,I
58 LD   E,B       -              BIT  3,B    bit 3,(iy+0)->b  IN   E,(C)
59 LD   E,C       -              BIT  3,C    bit 3,(iy+0)->c  OUT  (C),E
5A LD   E,D       -              BIT  3,D    bit 3,(iy+0)->d  ADC  HL,DE
5B LD   E,E       -              BIT  3,E    bit 3,(iy+0)->e  LD   DE,(&0000)
5C LD   E,H       LD   E,IXH     BIT  3,H    bit 3,(iy+0)->h  [neg]
5D LD   E,L       LD   E,IXL     BIT  3,L    bit 3,(iy+0)->l  [reti]
5E LD   E,(HL)    LD   E,(IX+0)  BIT  3,(HL) BIT  3,(IY+0)    IM   2
5F LD   E,A       -              BIT  3,A    bit 3,(iy+0)->a  LD   A,R
60 LD   H,B       LD   IXH,B     BIT  4,B    bit 4,(iy+0)->b  IN   H,(C)
61 LD   H,C       LD   IXH,C     BIT  4,C    bit 4,(iy+0)->c  OUT  (C),H
62 LD   H,D       LD   IXH,D     BIT  4,D    bit 4,(iy+0)->d  SBC  HL,HL
63 LD   H,E       LD   IXH,E     BIT  4,E    bit 4,(iy+0)->e  LD   (&0000),HL
64 LD   H,H       LD   IXH,IXH   BIT  4,H    bit 4,(iy+0)->h  [neg]
65 LD   H,L       LD   IXH,IXL   BIT  4,L    bit 4,(iy+0)->l  [retn]
66 LD   H,(HL)    LD   H,(IX+0)  BIT  4,(HL) BIT  4,(IY+0)    [im0]
67 LD   H,A       LD   IXH,A     BIT  4,A    bit 4,(iy+0)->a  RRD
68 LD   L,B       LD   IXL,B     BIT  5,B    bit 5,(iy+0)->b  IN   L,(C)
69 LD   L,C       LD   IXL,C     BIT  5,C    bit 5,(iy+0)->c  OUT  (C),L
6A LD   L,D       LD   IXL,D     BIT  5,D    bit 5,(iy+0)->d  ADC  HL,HL
6B LD   L,E       LD   IXL,E     BIT  5,E    bit 5,(iy+0)->e  LD   HL,(&0000)
6C LD   L,H       LD   IXL,IXH   BIT  5,H    bit 5,(iy+0)->h  [neg]
6D LD   L,L       LD   IXL,IXL   BIT  5,L    bit 5,(iy+0)->l  [reti]
6E LD   L,(HL)    LD   L,(IX+0)  BIT  5,(HL) BIT  5,(IY+0)    [im0]
6F LD   L,A       LD   IXL,A     BIT  5,A    bit 5,(iy+0)->a  RLD
70 LD   (HL),B    LD   (IX+0),B  BIT  6,B    bit 6,(iy+0)->b  IN   F,(C)
71 LD   (HL),C    LD   (IX+0),C  BIT  6,C    bit 6,(iy+0)->c  OUT  (C),F
72 LD   (HL),D    LD   (IX+0),D  BIT  6,D    bit 6,(iy+0)->d  SBC  HL,SP
73 LD   (HL),E    LD   (IX+0),E  BIT  6,E    bit 6,(iy+0)->e  LD   (&0000),SP
74 LD   (HL),H    LD   (IX+0),H  BIT  6,H    bit 6,(iy+0)->h  [neg]
75 LD   (HL),L    LD   (IX+0),L  BIT  6,L    bit 6,(iy+0)->l  [retn]
76 HALT           -              BIT  6,(HL) BIT  6,(IY+0)    [im1]
77 LD   (HL),A    LD   (IX+0),A  BIT  6,A    bit 6,(iy+0)->a  [ld i,i?]
78 LD   A,B       -              BIT  7,B    bit 7,(iy+0)->b  IN   A,(C)
79 LD   A,C       -              BIT  7,C    bit 7,(iy+0)->c  OUT  (C),A
7A LD   A,D       -              BIT  7,D    bit 7,(iy+0)->d  ADC  HL,SP
7B LD   A,E       -              BIT  7,E    bit 7,(iy+0)->e  LD   SP,(&0000)
7C LD   A,H       LD   A,IXH     BIT  7,H    bit 7,(iy+0)->h  [neg]
7D LD   A,L       LD   A,IXL     BIT  7,L    bit 7,(iy+0)->l  [reti]
7E LD   A,(HL)    LD   A,(IX+0)  BIT  7,(HL) BIT  7,(IY+0)    [im2]
7F LD   A,A       -              BIT  7,A    bit 7,(iy+0)->a  [ld r,r?]
80 ADD  A,B       -              RES  0,B    res 0,(iy+0)->b  -
81 ADD  A,C       -              RES  0,C    res 0,(iy+0)->c  -
82 ADD  A,D       -              RES  0,D    res 0,(iy+0)->d  -
83 ADD  A,E       -              RES  0,E    res 0,(iy+0)->e  -
84 ADD  A,H       ADD  A,IXH     RES  0,H    res 0,(iy+0)->h  -
85 ADD  A,L       ADD  A,IXL     RES  0,L    res 0,(iy+0)->l  -
86 ADD  A,(HL)    ADD  A,(IX+0)  RES  0,(HL) RES  0,(IY+0)    -
87 ADD  A,A       -              RES  0,A    res 0,(iy+0)->a  -
88 ADC  A,B       -              RES  1,B    res 1,(iy+0)->b  -
89 ADC  A,C       -              RES  1,C    res 1,(iy+0)->c  -
8A ADC  A,D       -              RES  1,D    res 1,(iy+0)->d  -
8B ADC  A,E       -              RES  1,E    res 1,(iy+0)->e  -
8C ADC  A,H       ADC  A,IXH     RES  1,H    res 1,(iy+0)->h  -
8D ADC  A,L       ADC  A,IXL     RES  1,L    res 1,(iy+0)->l  -
8E ADC  A,(HL)    ADC  A,(IX+0)  RES  1,(HL) RES  1,(IY+0)    -
8F ADC  A,A       -              RES  1,A    res 1,(iy+0)->a  -
90 SUB  A,B       -              RES  2,B    res 2,(iy+0)->b  -
91 SUB  A,C       -              RES  2,C    res 2,(iy+0)->c  -
92 SUB  A,D       -              RES  2,D    res 2,(iy+0)->d  -
93 SUB  A,E       -              RES  2,E    res 2,(iy+0)->e  -
94 SUB  A,H       SUB  A,IXH     RES  2,H    res 2,(iy+0)->h  -
95 SUB  A,L       SUB  A,IXL     RES  2,L    res 2,(iy+0)->l  -
96 SUB  A,(HL)    SUB  A,(IX+0)  RES  2,(HL) RES  2,(IY+0)    -
97 SUB  A,A       -              RES  2,A    res 2,(iy+0)->a  -
98 SBC  A,B       -              RES  3,B    res 3,(iy+0)->b  -
99 SBC  A,C       -              RES  3,C    res 3,(iy+0)->c  -
9A SBC  A,D       -              RES  3,D    res 3,(iy+0)->d  -
9B SBC  A,E       -              RES  3,E    res 3,(iy+0)->e  -
9C SBC  A,H       SBC  A,IXH     RES  3,H    res 3,(iy+0)->h  -
9D SBC  A,L       SBC  A,IXL     RES  3,L    res 3,(iy+0)->l  -
9E SBC  A,(HL)    SBC  A,(IX+0)  RES  3,(HL) RES  3,(IY+0)    -
9F SBC  A,A       -              RES  3,A    res 3,(iy+0)->a  -
A0 AND  B         -              RES  4,B    res 4,(iy+0)->b  LDI 
A1 AND  C         -              RES  4,C    res 4,(iy+0)->c  CPI 
A2 AND  D         -              RES  4,D    res 4,(iy+0)->d  INI 
A3 AND  E         -              RES  4,E    res 4,(iy+0)->e  OTI 
A4 AND  H         AND  IXH       RES  4,H    res 4,(iy+0)->h  -
A5 AND  L         AND  IXL       RES  4,L    res 4,(iy+0)->l  -
A6 AND  (HL)      AND  (IX+0)    RES  4,(HL) RES  4,(IY+0)    -
A7 AND  A         -              RES  4,A    res 4,(iy+0)->a  -
A8 XOR  B         -              RES  5,B    res 5,(iy+0)->b  LDD 
A9 XOR  C         -              RES  5,C    res 5,(iy+0)->c  CPD 
AA XOR  D         -              RES  5,D    res 5,(iy+0)->d  IND 
AB XOR  E         -              RES  5,E    res 5,(iy+0)->e  OTD 
AC XOR  H         XOR  IXH       RES  5,H    res 5,(iy+0)->h  -
AD XOR  L         XOR  IXL       RES  5,L    res 5,(iy+0)->l  -
AE XOR  (HL)      XOR  (IX+0)    RES  5,(HL) RES  5,(IY+0)    -
AF XOR  A         -              RES  5,A    res 5,(iy+0)->a  -
B0 OR   B         -              RES  6,B    res 6,(iy+0)->b  LDIR
B1 OR   C         -              RES  6,C    res 6,(iy+0)->c  CPIR
B2 OR   D         -              RES  6,D    res 6,(iy+0)->d  INIR
B3 OR   E         -              RES  6,E    res 6,(iy+0)->e  OTIR
B4 OR   H         OR   IXH       RES  6,H    res 6,(iy+0)->h  -
B5 OR   L         OR   IXL       RES  6,L    res 6,(iy+0)->l  -
B6 OR   (HL)      OR   (IX+0)    RES  6,(HL) RES  6,(IY+0)    -
B7 OR   A         -              RES  6,A    res 6,(iy+0)->a  -
B8 CP   B         -              RES  7,B    res 7,(iy+0)->b  LDDR
B9 CP   C         -              RES  7,C    res 7,(iy+0)->c  CPDR
BA CP   D         -              RES  7,D    res 7,(iy+0)->d  INDR
BB CP   E         -              RES  7,E    res 7,(iy+0)->e  OTDR
BC CP   H         CP   IXH       RES  7,H    res 7,(iy+0)->h  -
BD CP   L         CP   IXL       RES  7,L    res 7,(iy+0)->l  -
BE CP   (HL)      CP   (IX+0)    RES  7,(HL) RES  7,(IY+0)    -
BF CP   A         -              RES  7,A    res 7,(iy+0)->a  -
C0 RET  NZ        -              SET  0,B    set 0,(iy+0)->b  -
C1 POP  BC        -              SET  0,C    set 0,(iy+0)->c  -
C2 JP   NZ,&0000  -              SET  0,D    set 0,(iy+0)->d  -
C3 JP   &0000     -              SET  0,E    set 0,(iy+0)->e  -
C4 CALL NZ,&0000  -              SET  0,H    set 0,(iy+0)->h  -
C5 PUSH BC        -              SET  0,L    set 0,(iy+0)->l  -
C6 ADD  A,&00     -              SET  0,(HL) SET  0,(IY+0)    -
C7 RST  &00       -              SET  0,A    set 0,(iy+0)->a  -
C8 RET  Z         -              SET  1,B    set 1,(iy+0)->b  -
C9 RET            -              SET  1,C    set 1,(iy+0)->c  -
CA JP   Z,&0000   -              SET  1,D    set 1,(iy+0)->d  -
CB **** CB ****   -              SET  1,E    set 1,(iy+0)->e  -
CC CALL Z,&0000   -              SET  1,H    set 1,(iy+0)->h  -
CD CALL &0000     -              SET  1,L    set 1,(iy+0)->l  -
CE ADC  A,&00     -              SET  1,(HL) SET  1,(IY+0)    -
CF RST  &08       -              SET  1,A    set 1,(iy+0)->a  -
D0 RET  NC        -              SET  2,B    set 2,(iy+0)->b  -
D1 POP  DE        -              SET  2,C    set 2,(iy+0)->c  -
D2 JP   NC,&0000  -              SET  2,D    set 2,(iy+0)->d  -
D3 OUT  (&00),A   -              SET  2,E    set 2,(iy+0)->e  -
D4 CALL NC,&0000  -              SET  2,H    set 2,(iy+0)->h  -
D5 PUSH DE        -              SET  2,L    set 2,(iy+0)->l  -
D6 SUB  A,&00     -              SET  2,(HL) SET  2,(IY+0)    -
D7 RST  &10       -              SET  2,A    set 2,(iy+0)->a  -
D8 RET  C         -              SET  3,B    set 3,(iy+0)->b  -
D9 EXX            -              SET  3,C    set 3,(iy+0)->c  -
DA JP   C,&0000   -              SET  3,D    set 3,(iy+0)->d  -
DB IN   A,(&00)   -              SET  3,E    set 3,(iy+0)->e  -
DC CALL C,&0000   -              SET  3,H    set 3,(iy+0)->h  -
DD **** DD ****   -              SET  3,L    set 3,(iy+0)->l  -
DE SBC  A,&00     -              SET  3,(HL) SET  3,(IY+0)    -
DF RST  &18       -              SET  3,A    set 3,(iy+0)->a  -
E0 RET  PO        -              SET  4,B    set 4,(iy+0)->b  -
E1 POP  HL        POP  IX        SET  4,C    set 4,(iy+0)->c  -
E2 JP   PO,&0000  -              SET  4,D    set 4,(iy+0)->d  -
E3 EX   (SP),HL   EX   (SP),IX   SET  4,E    set 4,(iy+0)->e  -
E4 CALL PO,&0000  -              SET  4,H    set 4,(iy+0)->h  -
E5 PUSH HL        PUSH IX        SET  4,L    set 4,(iy+0)->l  -
E6 AND  &00       -              SET  4,(HL) SET  4,(IY+0)    -
E7 RST  &20       -              SET  4,A    set 4,(iy+0)->a  -
E8 RET  PE        -              SET  5,B    set 5,(iy+0)->b  -
E9 JP   (HL)      JP   (IX)      SET  5,C    set 5,(iy+0)->c  -
EA JP   PE,&0000  -              SET  5,D    set 5,(iy+0)->d  -
EB EX   DE,HL     -              SET  5,E    set 5,(iy+0)->e  -
EC CALL PE,&0000  -              SET  5,H    set 5,(iy+0)->h  -
ED **** ED ****   -              SET  5,L    set 5,(iy+0)->l  -
EE XOR  &00       -              SET  5,(HL) SET  5,(IY+0)    -
EF RST  &28       -              SET  5,A    set 5,(iy+0)->a  -
F0 RET  P         -              SET  6,B    set 6,(iy+0)->b  -
F1 POP  AF        -              SET  6,C    set 6,(iy+0)->c  -
F2 JP   P,&0000   -              SET  6,D    set 6,(iy+0)->d  -
F3 DI             -              SET  6,E    set 6,(iy+0)->e  -
F4 CALL P,&0000   -              SET  6,H    set 6,(iy+0)->h  -
F5 PUSH AF        -              SET  6,L    set 6,(iy+0)->l  -
F6 OR   &00       -              SET  6,(HL) SET  6,(IY+0)    -
F7 RST  &30       -              SET  6,A    set 6,(iy+0)->a  -
F8 RET  M         -              SET  7,B    set 7,(iy+0)->b  [z80]
F9 LD   SP,HL     -              SET  7,C    set 7,(iy+0)->c  [z80]
FA JP   M,&0000   -              SET  7,D    set 7,(iy+0)->d  [z80]
FB EI             -              SET  7,E    set 7,(iy+0)->e  ED_LOAD
FC CALL M,&0000   -              SET  7,H    set 7,(iy+0)->h  [z80]
FD **** FD ****   -              SET  7,L    set 7,(iy+0)->l  [z80]
FE CP   &00       -              SET  7,(HL) SET  7,(IY+0)    [z80]
FF RST  &38       -              SET  7,A    set 7,(iy+0)->a  ED_DOS
    
Notes on index registers
------------------------
Where DD and IX are mentioned, FD and IY may be substituted and vis versa.
    
Notes on Indexed Shift/Bit Operations
-------------------------------------
A shift or bit operation on an indexed byte in memory is done by prefixing
a CB opcode refering to (HL) with DD or FD to specify (IX+n) or (IY+n). 
If the CB opcode does not refer to (HL), slightly differing things happen.
The majority of Z80 CPUs execute them as shown; the shift or bit operation
is done on and indexed byte in memory, and then if the opcode does not
specify (HL) originally, the resultant byte is copied into the specified
register.  This is summarised with this example:
       CB 0x    RLC r          FD CB nn 0x     RLC (IY+nn)->r
       for x=0..5, 7 for r=B,C,D,E,H,L,A
  
Some CPUs allow access to the high and low halves of the index register,
if x is 4 or 5, the operation does RLC IYH or RLC IYH.
       CB 04   RLC H           FD CB nn 04     RLC IYH
       CB 05   RLC L           FD CB nn 05     RLC IYL
    
Some CPUs treat all the subcodes as accessing the indexed byte and nothing
else:
       CB 0x   RLC r           FD CB nn 0X     RLC (IY+nn)
                               for all x=0..7
    
Notes on ED opcodes
-------------------
J.G.Harston's !Z80Tube Z80 CoPro emulator includes the extra opcodes ED00
to ED0F to interface with the host.  G.A.Lunter's Z80 Spectrum emulator
includes the extra opcodes EDF8 to EDFF to interface to the host.


