---------------------------------------------------------------------
CP/M BOOT loaders that works with PEREX SHARP MZ-800 EMULATOR 
---------------------------------------------------------------------

Use them to boot CP/M floppies created from .MZD disk images with
STIMG.EXE or IMGBUILD.EXE ( these floppies are not "autobootable" 
from 'F'loppy disk menu )

Alternatively you can use them to boot every CP/M formatted floppy
with this emulator.

Run the bootloader like normal .mzf file ( game ) : 
go into 'C'asette tape menu, select the file and press ENTER. 
Before you do that, you should have SHARP MZ-800 CP/M formatted 
floppy already placed in disk drive. (see mzdhowto.txt for details 
on how to make CP/M formatted floppies)


cpmboot1.mzf	use it when you run SHARP MZ-800 emulator in regular
		MS-DOS or Windows9x "MS-DOS only" selection.
		(hold down F8 key while Windows booting to select 
		such option or restart them with "reboot MS-DOS"
		option.) 

cpmboot2.mzf    try this one if cpmload1.mzf does not boot the floppy
		you want to. 

-----------------------------------------------------------------------
  *NOTE*  These two booot loaders usually DO NOT boot when you are 
  running emulator in Windows9X window or shell (multitask mode).
------------------------------------------------------------------------


cpmwinb1.mzf    this one tries to boot the floppy when emulator is
		running in Windows9x task.

                - the emulated MZ-800 disk operations are very *unstable* 
		and go wrong when you run the emulator in Windows9x windowed
	        task -  usually you are not able to read certain files,
		CP/M will hang etc.

		Please use MS-DOS when you want to read/write floppies.




