
---------------------------------------------------------------------------
			MON80 Installation Menu
---------------------------------------------------------------------------
Increase the MP by 1  	 : 		Decrease the MP by 1  	 ; 
Increase the MP by 8  	 > 		Decrease the MP by 8  	 < 
Flip screen display   	 ^E 		Find Pattern 	      	 G 
Set Breakpoint 		 ^B 		Intelligent move	 I 
Continue 		 J 		Disassemble from PC	 L 
Set Memory pointer 	 M 		Find next pattern 	 N 
Follow relative offset 	 O 		Fill memory 		 P 
Load register from MP 	 T 		Read file 		 R 
Write file 		 W 		Show registers 		 S 
Disassemble a block 	 ^D 		Disassemble next page 	 ^N 
Reset breakpoint 	 ^R 		Restore after rel. off 	 U 
Restore after address 	 V 		Disassemble from MP 	 ^L 
Follow address at MP 	 X 		Single step 		 Z 
Repeat Loop 		 ^Z 		Continue interpreting 	 ^J 
Skip over instruction 	 ^X 		Delete last char 	 [DEL] 
Abort command 		 ^[ 		Return to CP/M 		 ^C 
---------------------------------------------------------------------------
L] 
Abort command 		 ^[ 		Return to CP/M 		 ^C 
---------------------------------------------